I want only ABCDE sensor, nothing else is acceptable